How to clean & maintain Polymer …….

Cleaning components, table tops, parts and accessories made with MGP is very simple:

* To clean everyday dirt and stains, use a cleaner such as Soft Scrub® and a nylon scrubby or stiff nylon brush. Scrub lightly; excess force can mar the finish.
* Persistent stains will usually go away if you soak the area with bleach (do not use 100% chlorine as used to treat swimming pools) and/or use a pressure washer.
* Also, stains and marks have been successfully removed with the following branded products: Goof Off®, Mr. Clean Magic Eraser®, GOJO Orange Pumice Hand Cleaner and Simple Green.
* To clean a petroleum stain such as grease or oil, use a citrus cleaner, alcohol or mineral spirits.
* In severe cases, spray petroleum-based stains with WD40®. Then use toluene or acetone and a white nylon scrub pad (colored pads release staining dyes when combined with acetone).
* Do not use MEK, turpentine or naphtha solvent.
* If a mark or stain won’t come out, you may lightly sand the area. Be careful and only work on the stained area because sanding will remove the matte finish.
* Any high-quality silicone marine caulk works well to replace old or worn caulking. Before caulking, the surface should be prepared by abrading it with a medium-grit sandpaper, then cleaning it with acetone, toluene or alcohol.

